**Instrument**CO2 Incubator **Model / Number**NU-5710  
 **Manufacturer**NuAire **Location**Life Sciences 250E **Instrument Description**NuAire direct heat incubators have built-in decontamination cycles, precise temperature and CO2 controls with electronic interface for user-friendly programming. These incubators have a large 5.7 cu.ft. interior chamber size directly heated with attached elements and a closed-loop air circulation system.  **User Charges**Not applicable  
  
**User Information**User must obtain permission from Laboratory PI to use these incubators. Any damage caused by the user is the responsibility of the user to repair or replace.